2.1

2.1.1 What is the logic voltage level, 3.3V or 5V?

Answer: In the data sheet provided for the L293/L293D in the page no. 4 in the table the logic voltage levels/supply voltage is greater than the minimum voltage that is 4.5V and can reach up-to 7V maximum, So by this we can conclude by this,

The logic voltage level is designed to operate in 5V.